Assessment Items

What are Assessment Items?

The assessment items are found in the Assessment Items tab of the Answer Network section in the Activity Wizard.

Most configurations in the answer network have corresponding assessment items. To assess certain items, place a check mark next to the item. The default behavior is to compare the student network configuration to what is defined in the answer network configuration. For more advanced activities, the assessment items can be replaced with a variable. In this case, the student network configuration is compared with the value defined in the variable.

How to Add Variables to the Items

Variables can only replace existing configured values. All leaf items can be replaced with a variable. A solid green dot indicates that a node has been replaced by a variable.

There are two options for replacing a configured value with a variable:
Option 1: Use the Variable Manager interface, click on <--
Option 2: Single click on the assessment item. A text field will pop up; replace the text with a variable.

Assessment Items and Values:

Assessment item values are loosely-typed; in fact, they are all of type String. However, some values follow this generic template:

Boolean: Less than or equal to 0 is false. Greater than or equal to 1 is true.
Numbers: A decimal (base 10) number.
IP Addresses: Must follow this format: 192.168.1.1; all digits between 0 and 255.
MAC Addresses: Must follow this format: ABCD.ABCD.ABCD; all digits must be hexadecimal.
Strings: Any regular string. A few string types require adherence to a specific format. This format is specified in the assessment item tree of the Activity Wizard.

Definition of Assessment Items and Values

These are the available nodes in Packet Tracer. The nodes follow a tree structure, where the leaf nodes are the nodes that can be graded. "<User Defined>" nodes take the name of a user configured value. For example, if a user configures a VLAN Name: "Engineering", the value "Engineering" will show in the runtime Assessment Tree but in this table, it will show as "<User Defined>."

AaaProcess | AclProcess | AclV6Process | AcsServerProcess | BgpProcess | Category | Cbac | CbacProcess | CbacProtocol | CdpProcess | ClassMapManager | ClientGroup | CMEProcess | CryptoMapSeq | CryptoMapSet | CustomQueueInfo | CustomQueueManager | DialPeer | DhcpPool | DhcpServerProcess | DhcpV6ClientProcess | DhcpV6LocalPrefixPool | DhcpV6Pool | DhcpV6ServerMainProcess | DhcpV6ServerProcess | DnsClient | DnsServerProcess | DynamicCryptoMap | EasyVpnServer | EigrpMainProcess | EigrpProcess | EigrpV6MainProcess | EigrpV6Process | EmailClient | EmailServer | EmailUser | Ephone | EphoneDirectory | FileManager | FtpServerProcess | GreProcess | HttpServer | HttpsServer | IcmpSignature | IkePolicy | IpsecPeer | IpsecProcess | IpsProcess | NatProcess | NatV6Process | NdProcess | NtpClientProcess | NtpServerProcess | OspfMainProcess | OspfProcess | OspfV3MainProcess | OspfV3Process | ParserView | ParserViewManager | PolicyMapManager | PolicyMapQosClass | PolicyMapZfwClass | PortKeepAliveProcess | PortSecurity | PppoeServer | PriorityQueueManager | PrivilegeManager | QueueProtocol | RadiusClientProcess | RadiusServerProcess | RipProcess | RipV6MainProcess | RipV6Process | RoutingProcess | RoutingProcessV6 | Settings | Security | Signature | SnmpAgent | Signature | SshServerProcess | StpMainProcess | SyslogClient | SyslogServer | TacacsClientProcess | TcpProcess | TelephonyService | TerminalLine | TftpServer | TransformSet | TunnelInterface | VirtualTemplateInterface | VirtualTemplateManager | VpdnGroup | VpnIpPool | VtpProcess | WirelessClientProcess | WirelessCommon | WirelessServerManager | WirelessServerPortData | WirelessServerProcess | ZfwProcess | ZonePair |
AccessPoint | AnalogPhone | Bridge | CableModem | CiscoDevice | Cloud | CloudPotsPort | CloudSerialPort | Console | Device | DslModem | EtherChannel | EtherChannelManager | FRSubInterface | HomeVoip | HostPort | Hub | IPPhone | Laptop | MultiLayerSwitch | MURemoteNetwork | Network | Pc | Pda | Printer | Port | RoutedSwitchPort | Router | RouterPort | Server | Switch | SwitchPort | TabletPC | TerminalLineDevice | TV | WiredEndDevice | WirelessRouter |

AaaProcess - up
Name | Node Type | Variable Type
AAA | Head |
New-model | Leaf | Number
Authentication | Head |
Authen Command <User Defined> | Leaf | String
Authorization | Head |
Authorize Command <User Defined> | Leaf | String

AcsServerProcess - up
Name | Node Type | Variable Type
ACS | Head |
ACS Enabled | Leaf | Boolean
Network Configuration | Head |
Client <User Defined> | Head |
Client IP | Leaf | IP Address
Client | Leaf | String
Secret String | Leaf | String
Server Type | Leaf | Number
User Setup | Head |
User <User Defined> | Head |
User Description | Leaf | String
User Name | Leaf | String
User Password | Leaf | String

RadiusClientProcess - up
Name | Node Type | Variable Type
RADIUS Client | Head |
RADIUS Server Hosts | Head |
<User Defined> | Leaf | Number
RADIUS server key | Leaf | String

RadiusServerProcess - up
Name | Node Type | Variable Type
RADIUS Server | Head |
Port | Leaf | Number

TacacsClientProcess - up
Name | Node Type | Variable Type
TACACS Client | Head |
TACACS Server Hosts | Head |
<User Defined> | Leaf | String
TACACS server key | Leaf | String

AclProcess - up
Name | Node Type | Variable Type
ACL | Head |
<User Defined> | Leaf | String

AclV6Process - up
Name | Node Type | Variable Type
ACLV6 | Head |
<User Defined> | Leaf | String

Cbac - up
Name | Node Type | Variable Type
Inspect name <User Defined> | Head |
Name | Leaf | String
Protocols | Head |
<CbacProtocol> | Head |

CbacProcess - up
Name | Node Type | Variable Type
Firewall | Head |
IP Inspect Names | Head |
<Cbac> | Head |
Global Alert | Leaf | Number
Global Audit Trail | Leaf | Number
DNS Timeout | Leaf | Number
FIN-WAIT Time | Leaf | Number
SYN-WAIT Time | Leaf | Number
UDP Idle Time | Leaf | Number
TCP Idle Time | Leaf | Number
MAX Incomplete High | Leaf | Number
MAX Incomplete Low | Leaf | Number
One Minute High | Leaf | Number
One Minute Low | Leaf | Number

CbacProtocol - up
Name | Node Type | Variable Type
Protocol <User Defined> | Head |
Protocol name | Leaf | String
Alert | Leaf | Number
Audit trail | Leaf | Number
Timeout | Leaf | Number

CdpProcess - up
Name | Node Type | Variable Type
CDP | Head |
CDP Enabled | Leaf | Boolean

DhcpPool - up
Name | Node Type | Variable Type
Pool <User Defined> | Head |
IPs | Leaf | String
Name | Leaf | String
DNS Server | Leaf | String
Default Gateway | Leaf | String
Start IP address | Leaf | String
Subnet mask | Leaf | String
Max Users | Leaf | Number
TFTP Server | Leaf | IP Address

DhcpServerProcess - up
Name | Node Type | Variable Type
DHCP | Head |
DHCP Enable | Leaf | Boolean
Pools | Head |
<DhcpPool> | Head |
Excluded Addresses | Head |
<User Defined> | Leaf | String

DhcpV6ClientProcess - up
Name | Node Type | Variable Type
DHCPV6 Client | Head |
DHCPV6 Client PD Name | Leaf | String

DhcpV6LocalPrefixPool - up
Name | Node Type | Variable Type
Local Pool Name <User Defined> | Head |
<User Defined> | Head |
Local Pool Name | Leaf | String
Prefix | Leaf | String
Prefix Length | Leaf | Number
Sub Prefix Length | Leaf | Number

DhcpV6Pool - up
Name | Node Type | Variable Type
Pool Name <User Defined> | Head |
<User Defined> | Head |
Pool Name | Leaf | String
DNS | Leaf | String
Domain Name | Leaf | String
Prefix Delegations | Head |
Prefix Delegations <User Defined> | Head |
Prefix Delegations | Leaf | String
DUID | Leaf | MAC Address
Static Preferred Lifetime | Leaf | Number
Static Valid Lifetime | Leaf | Number
Prefix Delegation Pool | Head |
Name <User Defined> | Head |
Name | Leaf | String
Dynamic Preferred Lifetime | Leaf | Number
Dynamic Valid Lifetime | Leaf | Number

DhcpV6ServerMainProcess - up
Name | Node Type | Variable Type
DHCPv6 | Head |
DHCPv6 Pools | Head |
<DhcpV6Pool> | Head |
Local Pools | Head |
<DhcpV6LocalPrefixPool> | Head |

DhcpV6ServerProcess - up
Name | Node Type | Variable Type
DHCPv6 Server | Head |
DHCPv6 Server Pool Name | Leaf | String

DnsClient - up
Name | Node Type | Variable Type
DNS | Head |
IP Domain Lookup | Leaf | Boolean
IP Domain Name | Leaf | String
IP Name Server | Leaf | IP Address
IPv6 Name Server | Leaf | IP Address
IP Host Header | Head |
Host <User Defined> | Leaf | String
IPv6 Host Header | Head |
Host <User Defined> | Leaf | String

DnsServerProcess - up
Name | Node Type | Variable Type
DNS Server | Head |
DNS Enable | Leaf | Boolean
Resource Records | Head |
Record <User Defined> | Head |
A Records | Head |
Address | Leaf | IP Address
NS Records | Head |
Server name | Leaf | String
SOA Records | Head |
SOA Record <User Defined> | Head |
Primary Server Name | Leaf | String
Mailbox | Leaf | String
Min TTL | Leaf | Number
Refresh Time | Leaf | Number
Retry Time | Leaf | Number
Expire Time | Leaf | Number
CNAME Records | Head |
Hostname | Leaf | String

ClientGroup - up
Name | Node Type | Variable Type
Group <User Defined> | Head |
Name | Leaf | String
Key | Leaf | String
Pool name | Leaf | String
Netmask | Leaf | String

DynamicCryptoMap - up
Name | Node Type | Variable Type
Map <User Defined> | Head |
Name | Leaf | String
Sequence number | Leaf | String
Crypto IpSec Transform Sets | Head |
<TransformSet> | Head |
Reverse-route | Leaf | Number

EasyVpnServer - up
Name | Node Type | Variable Type
Easy VPN Server | Head |
IP Local Pools | Head |
<VpnIpPool> | Head |
Client Configuration Groups | Head |
<ClientGroup> | Head |

VpnIpPool - up
Name | Node Type | Variable Type
Pool <User Defined> | Head |
Name | Leaf | String
Start IP | Leaf | String
End IP | Leaf | String

FileManager - up
Name | Node Type | Variable Type
Files | Head |
<User Defined Directory> | Head |
<User Defined File> | Leaf | String

FtpServerProcess - up
Name | Node Type | Variable Type
FTP Server | Head |
FTP Enable | Leaf | Boolean
User Accounts | Head |
Account <User Defined> | Head |
User Name | Leaf | String
User Password | Leaf | String
User Permission | Leaf | String
Server Files | Head |
<User Defined> | Leaf | String

GreProcess - up
Name | Node Type | Variable Type
GRE | Head |
Interface Tunnels | Head |
<TunnelInterface> | Head |

TunnelInterface - up
Name | Node Type | Variable Type
Tunnel <User Defined> | Head |
Port number | Leaf | String
Source | Leaf | String
Destination | Leaf | String

HttpServer - up
Name | Node Type | Variable Type
HTTP Server | Head |
HTTP Enable | Leaf | Boolean
Server Files | Head |
<User Defined> | Leaf | String

HttpsServer - up
Name | Node Type | Variable Type
HTTPS Server | Head |
HTTPS Enable | Leaf | Boolean

Category - up
Name | Node Type | Variable Type
Category <User Defined> | Head |
NAME | Leaf | String
Retired | Leaf | Number

Signature - up
Name | Node Type | Variable Type
Signature | Head |
Enabled | Leaf | Number
Retired | Leaf | Number

IcmpSignature - up
Name | Node Type | Variable Type
<Signature> | Head |
Icmp Signature ID | Leaf | Number
Icmp Sub ID | Leaf | Number

IpsProcess - up
Name | Node Type | Variable Type
IPS | Head |
Config Location Retries | Leaf | Number
Config Location | Leaf | String
Ips List | Head |
IPS Name <User Defined> | Head |
IPS Name | Leaf | String
Ips List | Leaf | String
Signature Categories | Head |
<Category> | Head |
<IcmpSignature> | Head |
Notify Log | Leaf | Number

Signature - up
Name | Node Type | Variable Type
Signature | Head |
Enabled | Leaf | Number
Retired | Leaf | Number

EmailClient - up
Name | Node Type | Variable Type
Email Client | Head |
<EmailUser> | Head |

EmailServer - up
Name | Node Type | Variable Type
Email Server | Head |
SMTP Service Enabled | Leaf | Boolean
POP3 Service Enabled | Leaf | Boolean
Domain Name | Leaf | String
Users | Head |
User <User Defined> | Head |
User Name | Leaf | String
User Password | Leaf | String

EmailUser - up
Name | Node Type | Variable Type
Email User | Head |
Name | Leaf | String
Email | Leaf | String
Incoming Mail Server | Leaf | String
Outgoing Mail Server | Leaf | String
User Name | Leaf | String
User Password | Leaf | String

NatProcess - up
Name | Node Type | Variable Type
NAT | Head |
Pools | Head |
Pool Name <User Defined> | Leaf | String
Inside Source List | Head |
NAT Source Setting <User Defined> | Leaf | String
Outside Source List | Head |
NAT Source Setting <User Defined> | Leaf | String
Inside Source Static | Head |
NAT Source Setting <User Defined> | Leaf | String
Outside Source Static | Head |
NAT Source Setting <User Defined> | Leaf | String

NatV6Process - up
Name | Node Type | Variable Type
NATV6 | Head |
Pools | Head |
<User Defined V6V4> | Leaf | String
<User Defined V4V6> | Leaf | String
Prefix | Head |
Prefix IP | Leaf | IP Address
Prefix Mask | Leaf | IP Address
Inside Source List | Head |
<User Defined V4V6> | Leaf | String
<User Defined V6V4> | Leaf | String
Inside Source Static | Head |
Name | Leaf | String

NdProcess - up
Name | Node Type | Variable Type
NDV6 | Head |
General Prefixes | Head |
General Prefix <User Defined> | Leaf | String
Neighbors | Head |
Neighbor <User Defined> | Head |
IPv6 Address | Leaf | IP Address
Mac Address | Leaf | MAC Address

NtpClientProcess - up
Name | Node Type | Variable Type
NTP Client | Head |
NTP Authenticate | Leaf | Number
Update Calendar | Leaf | Number
Authentication Keys | Head |
Key <User Defined> | Head |
Name | Leaf | String
Password | Leaf | String
Trusted Keys | Head |
Key | Leaf | Number
NTP Server Information | Head |
Address | Leaf | IP Address
Key | Leaf | String

NtpServerProcess - up
Name | Node Type | Variable Type
NTP Server | Head |
Service | Leaf | Boolean
Authentication | Leaf | Number
Key | Leaf | Number
Password | Leaf | String

PppoeServer - up
Name | Node Type | Variable Type
PPPOE Server | Head |
<VirtualTemplateManager> | Leaf | Boolean

VirtualTemplateManager - up
Name | Node Type | Variable Type
Virtual Template | Head |
Interfaces | Head |
<VirtualTemplateInterface> | Head |
VPDN Enable | Leaf | Boolean
VPDN Groups | Head |
<VpdnGroup> | Head |

VirtualTemplateInterface - up
Name | Node Type | Variable Type
Virtual Template Interface | Head |
IP Unnumbered Enabled | Leaf | String
Default IP Address Pool | Leaf | String
PPP CHAP Hostname | Leaf | String
PPP CHAP Password | Leaf | String
PPP Authentication | Leaf | Number

VpdnGroup - up
Name | Node Type | Variable Type
VPDN Group | Head |
Group Name | Leaf | String
Dial-in | Leaf | Boolean
Virtual Template | Leaf | Number
Protocol PPPOE | Leaf | Boolean

ClassMapManager - up
Name | Node Type | Variable Type
Class Maps | Head |
Class Map List | Head |
<User Defined> | Head |
Map Type | Leaf | Number
Statements | Head |
<User Defined> | Leaf | String

CustomQueueInfo - up
Name | Node Type | Variable Type
Custom Queue Info <User Defined> | Head |
Protocol List | Head |
<QueueProtocol> | Head |
Queues Infos | Head |
Queue Info | Leaf | String
Default Queue | Leaf | String

CustomQueueManager - up
Name | Node Type | Variable Type
Custom Queues | Head |
Custom Queue Info List | Head |
<CustomQueueInfo> | Head |

PolicyMapManager - up
Name | Node Type | Variable Type
Policy Maps | Head |
Policy Map List | Head |
Policy Map <User Defined> | Head |
Policy Map Name | Leaf | String
Policy Map Type | Leaf | Number
<PolicyMapQosClass | PolicyMapZfwClass> | Head |

PolicyMapQosClass - up
Name | Node Type | Variable Type
QoS Class <User Defined> | Head |
Map Name | Leaf | String
Bandwidth | Leaf | Number
Queue Limit | Leaf | Number
Priority | Leaf | Number
Service Policy | Leaf | String

PriorityQueueManager - up
Name | Node Type | Variable Type
Priority Queue | Head |
Priority List | Head |
<User Defined> | Head |
Protocol | Leaf | String
Queue Limit | Head |
High | Leaf | String
Medium | Leaf | String
Normal | Leaf | String
Low | Leaf | String
Default | Leaf | String

QueueProtocol - up
Name | Node Type | Variable Type
Queue Protocol | Head |
IP | Leaf | Number
IPv6 | Leaf | Number
Keyword | Leaf | Number
Key Value | Leaf | Number
Queue Index | Leaf | Number

BgpProcess - up
Name | Node Type | Variable Type
BGP | Head |
Autonomous System | Leaf | Number
Router ID | Leaf | IP Address
Log Neighbor Changes | Leaf | Boolean
Redistribute-internal | Leaf | Boolean
Networks | Head |
Route <User Defined> | Leaf | String
Neighbors | Leaf | Boolean
<User Defined> | Leaf | IP Address
Autonomous System | Leaf | Number
Next-Hop-Self | Leaf | Boolean
Timers | Head |
Keepalive | Leaf | Number
Holdtime | Leaf | Number
Synchronization | Leaf | Boolean
Redistribution | Head |
<User Defined> | Leaf | String

EigrpMainProcess - up
Name | Node Type | Variable Type
EIGRP | Head |
<EigrpProcess> | Head |

EigrpProcess - up
Name | Node Type | Variable Type
Autonomous System <User Defined> | Head |
Auto Summary | Leaf | Number
Networks | Head |
Route <User Defined> | Leaf | IP Address
Passive Interface | Head |
Default | Leaf | Number
<User Defined> | Leaf | String
Metrics | Leaf | String
Variance | Leaf | Number
Redistribution | Head |
<User Defined> | Leaf | String

OspfMainProcess - up
Name | Node Type | Variable Type
OSPF | Head |
<OspfProcess> | Head |

OspfProcess - up
Name | Node Type | Variable Type
Process ID <User Defined> | Head |
Area Authentication | Head |
Area <User Defined> | Leaf | Number
Area | Head |
Area <User Defined> | Leaf | Number
Area Status | Leaf | String
Default Cost | Leaf | Number
Virtual Link | Head |
<User Defined> | Leaf | String
Default Information | Leaf | Number
Log Adjacency Changes | Leaf | String
Passive Interface | Head |
Default | Leaf | Number
<User Defined> | Leaf | String
Networks | Head |
Route <User Defined> | Head |
Redistribution | Head |
<User Defined> | Leaf | String
Router ID | Leaf | String

RipProcess - up
Name | Node Type | Variable Type
RIP | Head |
Version | Leaf | Number
Auto Summary | Leaf | Number
Default Information Originate | Leaf | Boolean
Redistribution | Head |
<User Defined> | Leaf | String
Timers | Leaf | String
Networks | Head |
Route <User Defined> | Leaf | String
Passive Interface | Head |
Default | Leaf | Number
<User Defined> | Leaf | String

RoutingProcess - up
Name | Node Type | Variable Type
Routes | Head |
(deprecated) Static Routes | Head |
Route <User Defined> | Leaf | String
Static Routes | Head |
Route <User Defined> | Leaf | String
Default Networks | Head |
<User Defined> | Leaf | IP Address
IP Routing | Leaf | Boolean
Forward Protocols | Head |
<User Defined> | Leaf | String

EigrpV6MainProcess - up
Name | Node Type | Variable Type
EIGRPV6 | Head |
<EigrpV6Process> | Head |

EigrpV6Process - up
Name | Node Type | Variable Type
EIGRPv6 <User Defined> | Head |
Metrics | Leaf | String
Shutdown | Leaf | Number
Router ID | Leaf | IP Address
Redistribution | Head |
<User Defined> | Leaf | String

OspfV3MainProcess - up
Name | Node Type | Variable Type
OSPFV6 | Head |
<OspfV3Process> | Head |

OspfV3Process - up
Name | Node Type | Variable Type
OSPFv6 <User Defined> | Head |
Area | Head |
Area <User Defined> | Head |
Area Status | Leaf | String
Default Cost | Leaf | Number
Virtual Link | Head |
<User Defined> | Leaf | String
Log Adjacency Changes | Leaf | Number
Passive Interface | Head |
Default | Leaf | Number
<User Defined> | Leaf | String
Shutdown | Leaf | Number
Redistribution | Head |
<User Defined> | Leaf | String

RipV6MainProcess - up
Name | Node Type | Variable Type
RIPV6 | Head |
<RipV6Process> | Head |

RipV6Process - up
Name | Node Type | Variable Type
RIPv6 <User Defined> | Head |
Distance | Leaf | Number
Redistribution | Head |
<User Defined> | Leaf | String
ShutDown | Leaf | Number

RoutingProcessV6 - up
Name | Node Type | Variable Type
Routesv6 | Head |
IPv6 Unicast Routing | Leaf | Number
(deprecated) Static Routes | Head |
<User Defined> | Leaf | String
Static Routes | Head |
<User Defined> | Leaf | String
Default Networks | Head |
<User Defined> | Leaf | IP Address

Security - up
Name | Node Type | Variable Type
Security | Head |
Crypto Key Set | Leaf | String
Boot Config | Leaf | String
Boot Image | Leaf | String
Modulus Bits | Leaf | Number

SnmpAgent - up
Name | Node Type | Variable Type
SNMP | Head |
SNMP Communities | Head |
Community <User Defined> | Leaf | Number

SshServerProcess - up
Name | Node Type | Variable Type
SSH Server | Head |
SSH Version | Leaf | Number
SSH Authentication-retries | Leaf | Number
SSH Timeout | Leaf | Number

StpMainProcess - up
Name | Node Type | Variable Type
STP | Head |
VLANs | Head |
<User Defined> | Head |
VLAN Number | Leaf | Number
Priority | Leaf | Number
RSTP | Leaf | Number
PortFast Default | Leaf | Number

PortSecurity - up
Name | Node Type | Variable Type
Port Security | Head |
Enabled | Leaf | Boolean
Static MACs | Head |
<User Defined> | Leaf | MAC Address
Port Security Violation | Leaf | Number
Max Static MACs | Leaf | Number
Sticky Enabled | Leaf | Boolean
Sticky MACs | Head |
<User Defined> | Leaf | MAC Address

SyslogClient - up
Name | Node Type | Variable Type
SYSLOG Client | Head |
Server Addresses | Head |
Address | Leaf | String

SyslogServer - up
Name | Node Type | Variable Type
SYSLOG Server | Head |
Service | Leaf | Boolean

TcpProcess - up
Name | Node Type | Variable Type
TCP | Head |
Service Nagle | Leaf | Boolean
TCP MSS | Leaf | Number

TftpServer - up
Name | Node Type | Variable Type
TFTP | Head |
TFTP Enable | Leaf | Boolean
ServerFiles | Head |
<User Defined> | Leaf | String

CMEProcess - up
Name | Node Type | Variable Type
Call Manager Express | Head |
Dial Peers | Head |
<DialPeer> | Head |
<TelephonyService> | Head |
EPhones | Head |
<Ephone> | Head |
EPhone Directories | Head |
<EphoneDirectory> | Head |

DialPeer - up
Name | Node Type | Variable Type
Dial Peer <User Defined> | Head |
Tag Number | Leaf | Number
Destination Pattern | Leaf | Number
Session Target | Leaf | IP Address

Ephone - up
Name | Node Type | Variable Type
EPhone <User Defined> | Head |
Number | Leaf | Number
MAC Address | Leaf | MAC Address
Buttons | Head |
Button <User Defined> | Head |
Button | Leaf | Number
<EphoneDirectory> | Head |

EphoneDirectory - up
Name | Node Type | Variable Type
EPhone Directory <User Defined> | Head |
Directory Number | Leaf | Number
Directory Line Number | Leaf | String

TelephonyService - up
Name | Node Type | Variable Type
Telephony Service | Head |
Auto Assign Commands | Head |
Auto Assign <User Defined> | Leaf | String
Max Directory Number | Leaf | Number
Max EPhone Number | Leaf | Number
Source IP | Leaf | IP Address
Source Port | Leaf | Number

CryptoMapSeq - up
Name | Node Type | Variable Type
Sequence | Head |
Number | Leaf | String
Peers | Head |
<IpsecPeer> | Head |
Match address | Leaf | String

CryptoMapSet - up
Name | Node Type | Variable Type
Set | Head |
Name | Leaf | String
Respond | Leaf | String
Sequence List | Head |
<CryptoMapSeq> | Head |
Ports | Head |
Port | Leaf | Number

IkePolicy - up
Name | Node Type | Variable Type
Policy <User Defined> | Head |
Number <User Defined> | Leaf | Number
Authentication type | Leaf | String
Hash algorithm | Leaf | String
Encryption | Leaf | String
Group | Leaf | Number
Lifetime | Leaf | Number

IpsecPeer - up
Name | Node Type | Variable Type
Peer | Head |
Address | Leaf | String

IpsecProcess - up
Name | Node Type | Variable Type
IKE | Head |
Crypto ISAKMP Policy | Head |
<IkePolicy> | Head |
Crypto ISAKMP Key Address Pairs | Head |
<User Defined> | Leaf | String
Crypto IpSec Transform Sets | Head |
<TransformSet> | Head |
Crypto Map Sets | Head |
<CryptoMapSet> | Head |
Crypto Dynamic Maps | Head |
<DynamicCryptoMap> | Head |
ISAKMP Enable | Leaf | Number
Security Association | Leaf | Number

TransformSet - up
Name | Node Type | Variable Type
Set | Head |
Name | Leaf | String
AH Transform | Leaf | Number
ESP Authentication Transform | Leaf | Number
ESP Encryption Transform | Leaf | Number

VtpProcess - up
Name | Node Type | Variable Type
VTP | Head |
Domain Name | Leaf | String
VTP Mode | Leaf | Number
VTP Password | Leaf | String
VTP Version | Leaf | Number

WirelessClientProcess - up
Name | Node Type | Variable Type
<WirelessCommon> | Head |
Security Mode | Head |
User Id | Leaf | String
Password | Leaf | String

WirelessCommon - up
Name | Node Type | Variable Type
Wireless | Head |
SSID | Leaf | String
Security Mode | Head |
Authen Type | Leaf | Number
WEP Key | Leaf | String
PassPhrase | Leaf | String
Encryption Type | Leaf | Number

WirelessServerManager - up
Name | Node Type | Variable Type
Dot11 Configuration | Head |
SSID Configurations | Head |
SSID <User Defined> | Leaf | String
SSID name | Leaf | String
Authentication | Leaf | String
WPA key management | Leaf | Number
EAP method | Leaf | String
EAP list name | Leaf | String
Wpa-psk | Head |
Key entered as | Leaf | String
Unencrypted | Leaf | Number
Key | Leaf | Number
Dot11Radio Configurations | Head |
<WirelessServerPortData> | Head |

WirelessServerPortData - up
Name | Node Type | Variable Type
Dot11Radio | Head |
Bridge Group | Leaf | Number
Station Role | Leaf | Boolean
Speed | Leaf | String
Encryption | Head |
Key | Leaf | String
Size | Leaf | String
Type | Leaf | String
Hex String | Leaf | String
Mode WEP | Leaf | String
Mode Cipher | Leaf | String
SSID | Leaf | String

WirelessServerProcess - up
Name | Node Type | Variable Type
<WirelessCommon> | Head |
Security Mode | Head |
RADIUS Server IP | Leaf | String
RADIUS Shared Secret | Leaf | String
SSID BroadCast | Leaf | Number
Mac Filter Mode | Head |
Mode | Leaf | Boolean
Access Restriction | Leaf | Number
Mac Address List | Head |
Mac Address | Leaf | MAC Address

PolicyMapZfwClass - up
Name | Node Type | Variable Type
Inspect Class <User Defined> | Head |
Class Map | Leaf | String
Action | Leaf | Number

ZfwProcess - up
Name | Node Type | Variable Type
Zone Based Firewall | Head |
Zone Names | Head |
<User Defined> | Leaf | String
Zone Pairs | Head |
<ZonePair> | Head |

ZonePair - up
Name | Node Type | Variable Type
Zone Pair <User Defined> | Head |
Name | Leaf | String
Source Zone | Leaf | String
Destination Zone | Leaf | String
Service Policy | Leaf | String

Settings - up
Name | Node Type | Variable Type
Algorithm Settings | Head |
CBAC | Head |
Half-Open Session Multiplier | Leaf | Number
TCP | Head |
Maximum Number of Connections | Leaf | Number
Maximum Number of Open Sessions | Leaf | Number
Switching | Head |
Storm Control Multipler | Leaf | Number

PrivilegeManager - up
Name | Node Type | Variable Type
Command Privilege | Head |
Commands | Head |
Command | Leaf | String

ParserView - up
Name | Node Type | Variable Type
View | Head |
View name | Leaf | String
Secret | Leaf | String
Commands | Head |
Command | Leaf | String

ParserViewManager - up
Name | Node Type | Variable Type
Parser View | Head |
Views | Head |
<ParserView> | Head |

TerminalLine - up
Name | Node Type | Variable Type
RS232 | Console Line | VTY Line <User Defined> | | Head |
Speed | Leaf | Number
Data Bits | Leaf | Number
Parity | Leaf | Number
Stop Bits | Leaf | String
Flow Control | Leaf | Number
Transport Input | Leaf | Number
Transport Output | Leaf | Number
History Size | Leaf | Number
MOTD Banner | Leaf | Number
Login | Leaf | Number
Password | Leaf | String
AAA Method List Name | Leaf | String
Session Limit | Leaf | Number
Access Class In | Leaf | String
Access Class Out | Leaf | String
Exec-timeout | Leaf | Number
Logging Synch | Leaf | Number
Privilege Level | Leaf | Number
IPv6 Access-class In | Leaf | String
IPv6 Access-class Out | Leaf | String

AccessPoint - up
Name | Node Type | Variable Type
<Device> | Head |
<WirelessServerProcess> | Head |

AnalogPhone - up
Name | Node Type | Variable Type
<Device> | Head |

Bridge - up
Name | Node Type | Variable Type
<Device> | Head |

CableModem - up
Name | Node Type | Variable Type
<Device> | Head |

CiscoDevice - up
Name | Node Type | Variable Type
<AaaProcess> | Head |
Banner login | Leaf | String
Banner motd | Leaf | String
Boot System | Head |
<User Defined> | Leaf | String
<CdpProcess> | Head |
Clock Timezone | Leaf | String
Config-Register | Leaf | Number
<Console> | Head |
<DnsClient> | Head |
Enable Password | Leaf | String
Flash Files | Head |
<User Defined> | Leaf | String
FTP Passive | Leaf | Number
FTP Password | Leaf | String
FTP Username | Leaf | String
Host Name | Leaf | String
IP Domain Name | Leaf | String
Login Options | Head |
Login On Success | Leaf | Number
Login On Failure | Leaf | Number
Blocking | Head |
Enabled | Leaf | Boolean
Duration | Leaf | Number
Attempts | Leaf | Number
Period | Leaf | Number
<NtpClientProcess> | Head |
<RadiusClientProcess> | Head |
<Settings> | Head |
<Security> | Head |
Security Password Min-Length | Leaf | Number
Service Password Encryption | Leaf | Number
<SshServerProcess> | Head |
Startup Config | Leaf | Number
Static MAC | Head |
<User Defined> | Leaf | String
<SyslogClient> | Head |
<TacacsClientProcess> | Head |
<TerminalLine> | Head |
User Names | Head |
User Name | Leaf | String
VTY Lines | Head |
<TerminalLine> | Head |

Cloud - up
Name | Node Type | Variable Type
<Device> | Head |
Frame Relay Connections | Head |
<User Defined> | Leaf | String
DSL Connections | Head |
<User Defined> | Leaf | String
Cable Connections | Head |
<User Defined> | Leaf | String

Device - up
Name | Node Type | Variable Type
<User Defined> | Head |
Custom Model Name | Leaf | String
Custom Variables | Head |
<User Defined> | Leaf | String
Device Model | Leaf | String
Device Type | Leaf | Number
In Logical Shape | Leaf | String
In Physical Shape | Leaf | String
Ports | Head |
<Port> | Head |
Power | Leaf | Number
Authorization | Leaf | String

DslModem - up
Name | Node Type | Variable Type
<Device> | Head |

HomeVoip - up
Name | Node Type | Variable Type
<Device> | Head |
SCCP Server Address | Leaf | IP Address

Hub - up
Name | Node Type | Variable Type
<Device> | Leaf | Number

IPPhone - up
Name | Node Type | Variable Type
<Device> | Leaf | Number

Laptop - up
Name | Node Type | Variable Type
<Pc> | Head |

MultiLayerSwitch - up
Name | Node Type | Variable Type
<Router> | Head |
<EtherChannelManager> | Head |
MLS QoS Enabled | Leaf | Number

Pc - up
Name | Node Type | Variable Type
<TerminalLineDevice> | Head |
Accessories | Head |
Camera Connected | Leaf | Boolean
Headphone Connected | Leaf | Boolean
Microphone Connected | Leaf | Boolean
USB Hard Drive Connected | Leaf | Boolean
Default Gateway | Leaf | IP Address
Default Gateway IPv6 | Leaf | IP Address
DNS Server | Leaf | IP Address
DNS Server IPv6 | Leaf | IP Address
<EmailClient> | Head |
Files | Head |
C Directory | Head |
sampleFile.txt | Leaf | String
<User Defined> | Leaf | String
Desktop | Head |
sampleFile.txt | Leaf | String
<User Defined> | Leaf | String
<Settings> | Head |
<TerminalLine> | Head |
<WirelessClientProcess> | Head |

Pda - up
Name | Node Type | Variable Type
<Pc> | Head |

Printer - up
Name | Node Type | Variable Type
<Pc> | Head |

Router - up
Name | Node Type | Variable Type
<CiscoDevice> | Head |
<AclProcess> | Head |
<AclV6Process> | Head |
<CbacProcess> | Head |
<ClassMapManager> | Head |
<CMEProcess> | Head |
<CustomQueueManager> | Head |
<BgpProcess> | Head |
<CbacProcess> | Head |
<DhcpServerProcess> | Head |
<DhcpV6ServerMainProcess> | Head |
<EasyVpnServer> | Head |
<EigrpMainProcess> | Head |
<EigrpV6MainProcess> | Head |
<GreProcess> | Head |
<IpsecProcess> | Head |
<IpsProcess> | Head |
<NatProcess> | Head |
<NatV6Process> | Head |
<NdProcess> | Head |
<OspfMainProcess> | Head |
<OspfV3MainProcess> | Head |
<ParserViewManager> | Head |
<PolicyMapManager> | Head |
<PriorityQueueManager> | Head |
<PrivilegeManager> | Head |
<RipProcess> | Head |
<RipV6Process> | Head |
<RoutingProcess> | Head |
<RoutingProcessV6> | Head |
<SnmpAgent> | Head |
<SshServerProcess> | Head |
<Security> | Head |
<StpMainProcess> | Head |
<TcpProcess> | Head |
VLANS | Head |
<User Defined> | Head |
VLAN Name | Leaf | String
<VirtualTemplateManager> | Head |
<VtpProcess> | Head |
<WirelessServerManager> | Head |
<ZfwProcess> | Head |

Server - up
Name | Node Type | Variable Type
<Pc> | Head |
<AcsServerProcess> | Head |
<DhcpServerProcess> | Head |
<DnsServerProcess> | Head |
<EmailServer> | Head |
<FtpServerProcess> | Head |
<HttpServer> | Head |
<HttpsServer> | Head |
<NtpServerProcess> | Head |
<RadiusServerProcess> | Head |
<SyslogServer> | Head |
<TftpServer> | Head |
<EmailServer> | Head |

Switch - up
Name | Node Type | Variable Type
<CiscoDevice> | Head |
Default Gateway | Leaf | IP Address
<EtherChannelManager> | Head |
<SnmpAgent> | Head |
<StpMainProcess> | Head |
VLANS | Head |
<User Defined> | Leaf | String
VLAN Name | Leaf | String
<VtpProcess> | Head |

TabletPC - up
Name | Node Type | Variable Type
<Pc> | Head |

TerminalLineDevice - up
Name | Node Type | Variable Type
<Device> | Head |
Enable Secret | Leaf | String
Logging | Head |
Service timestamp debug | Leaf | Number
Service timestamp log | Leaf | Number
Logging console | Leaf | Number
Logging buffered | Leaf | Number
Logging On | Leaf | Number
Trap Debug | Leaf | Number

TV - up
Name | Node Type | Variable Type
<Device> | Head |

WiredEndDevice - up
Name | Node Type | Variable Type
<Pc> | Head |

WirelessRouter - up
Name | Node Type | Variable Type
<Device> | Head |
Default Gateway | Leaf | IP Address
<DhcpServerProcess> | Head |
DNS Server IP | Leaf | IP Address
Internet Connection | Leaf | Number
Password | Leaf | String
Remote Management | Leaf | Boolean
Single Port Forwarding | Head |
<User Defined> | Leaf | String
<WirelessServerProcess> | Head |

Console - up
Name | Node Type | Variable Type
<Port> | Head |

CloudPotsPort - up
Name | Node Type | Variable Type
<Port> | Head |
Phone Number | Leaf | String

CloudSerialPort - up
Name | Node Type | Variable Type
<Port> | Head |
Frame Relay | Head |
LMI Type | Leaf | Number
Sublinks | Head |
<User Defined> | Leaf | String

FRSubInterface - up
Name | Node Type | Variable Type
<RouterPort> | Head |
Type (Point-to-Point/ MultiPoint) | Leaf | Number
DLCI | Head |
DLCI <User Defined> | Leaf | Number

HostPort - up
Name | Node Type | Variable Type
<Port> | Head |
ARP Timeout | Leaf | Number
Auto Config | Leaf | Number
DHCP client enable | Leaf | Boolean
<DhcpV6ClientProcess>
IP Address | Leaf | IP Address
ip mtu | Leaf | Number
Ipv6 Address | Head |
IPv6 Enable | Leaf | Number
<User Defined> | Head |
IP Address | Leaf | IP Address
Prefix | Leaf | String
Type | Leaf | String
ipv6 mtu | Leaf | Number
Link Local | Leaf | IP Address
mtu | Leaf | Number
Subnet Mask | Leaf | IP Address

Port - up
Name | Node Type | Variable Type
<User Defined> | Head |
Bandwidth Auto Negotiate | Leaf | Number
Clock Rate | Leaf | Number
Description | Leaf | String
Duplex Auto Negotiate | Leaf | String
MAC Address | Leaf | MAC Address
Port Type | Leaf | Number
<PortKeepAliveProcess> | Head |
Power | Leaf | Number
Tx Ring Limit | Leaf | Number
(Wireless) Link to <User Defined> | Head |
Connects to <User Defined> | Leaf | String
DCE Port Name | Leaf | String
Type | Leaf | Number

PortKeepAliveProcess - up
Name | Node Type | Variable Type
Port Keepalive | Head |
Keepalive interval | Leaf | Number

RoutedSwitchPort - up
Name | Node Type | Variable Type
<SwitchPort | RouterPort> | Head |
SwitchPort | Leaf | Number

EtherChannel - up
Name | Node Type | Variable Type
<RoutedSwitchPort> | Head |
Channel group | Head |
Channel mode | Leaf | Number
Channel protocol | Leaf | Number

EtherChannelManager - up
Name | Node Type | Variable Type
EtherChannel | Head |
Load Balance Method | Leaf | Number

RouterPort - up
Name | Node Type | Variable Type
<HostPort> | Head |
802.1Q | Head |
VLAN ID | Leaf | Number
Native VLAN | Leaf | Number
Access-group In | Leaf | String
Access-group Out | Leaf | String
CDP Enabled | Leaf | Number
Crypto Map | Leaf | String
Bandwidth Info | Leaf | Number
Delay | Leaf | Number
<Dhcpv6ServerProcess> | Head |
EIGRP Hello Interval | Head |
Autonomous System <User Defined> | Leaf | Number
EIGRP Summary Addresses | Head |
Autonomous System <User Defined> | Head |
<User Defined> | Leaf | String
EIGRPv6 | Head |
EIGRPv6 <User Defined> Enabled | Leaf | Boolean
EIGRPV6 Hello Interval | Head |
Autonomous System <User Defined> | Leaf | Number
Eigrpv6 Summary Addresses | Head |
Autonomous System <User Defined> | Head |
<User Defined> | Leaf | String
Encapsulation | Leaf | String
Frame Relay | Head |
Encapsulation Type | Leaf | Number
LMI Type | Leaf | Number
IP Maps | Head |
<User Defined> | Leaf | String
Helper Addresses | Head |
Helper Address <User Defined> | Leaf | IP Address
Hold Queue | Leaf | Number
Ip Inspect In | Leaf | String
Ip Inspect Out | Leaf | String
Ips In | Leaf | String
Ips Out | Leaf | String
IPv6 NAT | Leaf | Number
IPv6 NAT Prefix | Leaf | String
IPv6 Traffic Filter In | Leaf | String
IPv6 Traffic Filter Out | Leaf | String
Keepalive | Leaf | Boolean
NAT Mode | Leaf | Number
OSPF Authentication | Leaf | Number
OSPF Authentication Key | Leaf | String
OSPF Cost | Leaf | Number
OSPF Dead Interval | Leaf | Number
OSPF Hello Interval | Leaf | Number
OSPF Message Digest Key | Head |
Key ID <User Defined> | Leaf | Number
Ospf Network Type | Leaf | Number
OSPF Priority | Leaf | Number
OSPFv3 | Head |
OSPFv3 Process ID | Leaf | Number
OSPFv3 Area ID | Leaf | String
OSPFv3 Instance ID | Leaf | Number
OSPFv3 Priority | Leaf | Number
OSPFv3 Dead Interval | Leaf | Number
OSPFv3 Hello Interval | Leaf | Number
OSPFv3 cost | Leaf | Number
PPP | Head |
Authentication | Leaf | Number
PPPOE Enabled | Leaf | Number
Priority Group | Custom Queue List | Fair Queue | Leaf | Number | Number | String
RIP Split Horizon | Leaf | Boolean
RIPv6 | Head |
RIPv6 <User Defined> Enabled | Leaf | Boolean
Route cef | Leaf | Boolean
Service Policy Input | Leaf | String
Service Policy Output | Leaf | String
Virtual Reassembly | Leaf | Number
Zone Member | Leaf | String

SwitchPort - up
Name | Node Type | Variable Type
<Port> | Head |
Access VLAN | Leaf | Number
Bpduguard | Leaf | Number
CDP Enabled | Leaf | Number
Dynamic Mode | Leaf | Number
Native VLAN | Leaf | Number
Nonegotiate | Leaf | Boolean
Port Mode | Leaf | Number
PortFast | Leaf | Number
<PortSecurity> | Head |
Root guard | Leaf | Number
Storm Control | Leaf | String
Trunk VLANs | Head |
<User Defined> | Leaf | String
Voice Vlan | Leaf | Number

Network - up
Name | Node Type | Variable Type
Network | Head |
<Device> | Head |
<MURemoteNetwork> | Head |

MURemoteNetwork - up
Name | Node Type | Variable Type
<Device> | Leaf | Number
Peer Address | Leaf | String
Peer Network Name | Leaf | String
Password | Leaf | String
Connected | Leaf | Boolean