Devices and Modules: Switches

All images on this page are thumbnails on which you can click to bring up a larger image.

Switch: 2950-24

The Cisco Catalyst 2950-24 is a member of the Cisco Catalyst 2950 series switch family. It is a standalone, fixed-configuration, managed 10/100 switch providing user connectivity for small- to mid-sized networks.

It does not support add-in modules.

Switch: 2950T-24

The Cisco Catalyst 2950T-24 is a member of the Catalyst 2950 Series Intelligent Ethernet Switch family. It is a fixed-configuration, standalone switch that provides wire-speed Fast Ethernet and Gigabit Ethernet connectivity for mid-sized networks.

It does not support add-in modules.

Switch: 2960-24TT

The Cisco Catalyst 2960-24TT is a member of the Catalyst 2960 Series Intelligent Ethernet Switch family. It is a fixed-configuration, standalone switch that provides wire-speed Fast Ethernet and Gigabit Ethernet connectivity for mid-sized networks.

It does not support add-in modules.

Switch: Switch-PT

The Switch-PT generic switch provides ten slots, one console port, and one auxiliary port.

PT-SWITCH-NM-1CE |  | The PT-SWITCH-NM-1CE features a single Ethernet port that can connect a LAN backbone which can also support either six PRI connections to aggregate ISDN lines, or 24 synchronous/asynchronous ports.
PT-SWITCH-NM-1CFE |  | The PT-SWITCH-NM-1CFE Module provides one Fast-Ethernet interface for use with copper media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
PT-SWITCH-NM-1CGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-SWITCH-NM-1CGE) provides Gigabit Ethernet copper connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.
PT-SWITCH-NM-1FFE |  | The PT-SWITCH-NM-1FFE Module provides one Fast-Ethernet interface for use with fiber media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet.
PT-SWITCH-NM-1FGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-SWITCH-NM-1FGE) provides Gigabit Ethernet optical connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.

Switch: 3560-24PS

The Cisco Catalyst 3560-24PS is a member of the Catalyst 3560 Series Intelligent Ethernet Switch family. It is a fixed-configuration, standalone switch that provides wire-speed Fast Ethernet and Gigabit Ethernet connectivity for mid-sized networks.

It does not support add-in modules.

Bridge-PT

This bridge provides two slots.

The bridge supports the same modules that the Switch-PT supports.